**S.K.D.A.V. GOVERNMENT POLYTECHNIC, ROURKELA.**

Telefax-0661-2420550, Website-www.skdavpolytech.ac.in,

Email-Id-principal\_skdav@rediffmail.com

Notice No.**188**/SGPR/Dt.**21/02/2018/**

**QUOTATION CALL NOTICE**

It is proposed to purchase of Equipments for Electronics & Telecommunication Department (As per List Enclosed) for the session 2017-18. Interested firms/suppliers /manufactures / authorized dealer may submit their quotation in sealed envelope super-scribed “QUOTATION FOR EQUIPMENTS OF E & TC DEPTT”. So as to reach the undersigned on or before 12.03.2018 by 11 AM. Documents relating to GST may be enclosed with the quotation. You are also requested to mention the make & Model of the item along with the rate.

The Quotations will be opened on 12.03.2018 at 12.00 PM. Quotationers or their representative with proper authorization letter may present at the time of opening of quotation.

The undersigned reserves the right to reject or accept any quotation/ all quotations without assigning any reason thereof.

-Sd-

Principal

SKDAV Government Polytechnic,

Rourkela

Memo No.\_\_\_\_ \_\_\_\_\_\_\_\_\_\_/.Dt\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_/

Copy to Notice Board of the Institution for information of public.

-Sd-

Principal

Memo No.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_/.Dt.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_/

Copy (2 copies each) to the General Manager, R.I Centre, Rkl, ADM, Rkl/Treasury officer special treasury Panposh, Rourkela/Sub Collector, Rourkela/P.D.D.R.D.A, Sundergarh with a request to display a copy of this quotation call notice in their respective office notice board.

-sd-

Principal

**PLC LAB INSTALLATION**

|  |  |
| --- | --- |
| **SL.NO.** | **NAME OF EQUIPMENT** |
| 1 | Open slotted PVC channel, Grey PVC-45mm\*45mm meter |
| 2 | Insulated ferrules, blue, yellow, red, black, grey ,white, green each |
| 3 | Cable ties, Smallest size |
| 4 | Cable glands, mounting thread size : standard, cable Diameter : 6-12cm, Mounting thread length : 5-7m |
| 5 | PLC Programmable Cable, PLC or USB type |
| 6 | DIN rail, Symmetric-Standard top hat 60-100c.m length |
| 7 | Panel Lamp with holder, 24V AC/DC, 6A-Panel mountable |
| 8 | Toggle switch (SPST), 24V AC/DC, 6A-Panel mountable |
| 9 | Rocker switch, 10A @ 250V AC-Bigger size |
| 10 | Push Button ,NO-Panel Mountable, NC-Panel Mountable |
| 11 | 3-core cable,6A,conductor area (0.75mm2) |
| 12 | Wire ( blue, yellow, red, black, grey ,white, green), 6A,conductor area (0.75mm2) |
| 13 | MCB-DIN rail mountable, 6A-10A,4 nos of pole |
| 14 | DIN rail mounted fuse terminal, 24V DC, 3A with fuse |
| 15 | DIN rail mounted terminal connectors, standard grey type-one way |
| 16 | SMPS, 3A-6A 24V DC O/P |
| 17 | 3-Phase Contractor, 440v, 4NOs and Auxiliary NO/NC |
| 18 | 3-Phase Ind. Motor, 5HP |
| 19 | PLC |
| 20 | Programmable Software Development |
| 21 | Cabinet-Panel Mount |